# Lab 5 Report

## Summary:

The difference between process 0 and process 1 is the ordering in which we arrange our receive and sends. Process 0 sends out before receiving and Process 1 receives before sending in our arrangement. The maximum bandwidth was achieved with a message size of 512 so the ideal buffer size is approximately 512 doubles.

![A close up of a sign

Description automatically generated]()